For 1990-2009 cars

#### Battery Fastener Tightening Specifications

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Hold-down Retainer Bolt | 15 | 11 | --
Negative Cable-to-A/C Compressor Bracket Bolt | 25 | 18 | --
Negative Cable-to-Battery Clamp Bolt | 6 | -- | 53
Positive Cable-to-Battery Clamp Bolt | 6 | -- | 53

#### Starter Fastener Tightening Specifications

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Armature Bearing Housing Screw | 1.8 | -- | 16
Battery Cable Terminal Nut | 13 | -- | 115
Commutator End Shield Bolt | 5 | -- | 44
Engine Mount Bracket Bolt | 40 | 30 | --
Starter Bearing Housing Bolt | 1.8 | -- | 16
Starter Motor-to-Engine Bolt | 60 | 44 | --
Starter Solenoid Field Lead Nut | 8 | -- | 71
Starter Solenoid Screw | 5 | -- | 44
Starter Solenoid Terminal Nut | 4 | -- | 35

#### Generator Fastener Tightening Specifications

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Battery Terminal Nut | 8 | -- | 71
Cooling Duct Cap Screw | 1 | -- | 9
Field Coil Terminal Nut | 3.5 | -- | 31
Front Bearing Screw | 3 | -- | 27
Housing Bolt | 5 | -- | 44
Mounting Bolt (Upper/Lower) | 40 | 30 | --
Mounting Nut (Upper/Lower) | 40 | 30 | --
Pulley Nut | 65 | 48 | --
Voltage Regulator Screw | 1.5 | -- | 13

#### Ignition System Fastener Tightening Specifications

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Bracket, Bolt A/C Compressor Hose-to-Cylinder Head | 8 | -- | 71
Ignition Coil Bolt | 8 | -- | 71
Spark Plug | 25 | 19 | --
Throttle Cable Bracket-to-Intake Plenum Bolt | 8 | -- | 71
Wire Harness-to-Intake Plenum Bolt | 8 | -- | 71