For 1990-2009 cars

Table 1: | Gauge Cluster Connector
Table 2: | Instrument Cluster Connector

#### Gauge Cluster Connector

Connector Part Information |

• | ZF 26 - 1

• | 26 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/YEL | XB3 | Washer Solvent Level Signal
2 | YEL/RED | BA2 | Brake Pad Wear Signal
3 | BRN/BLU | XP2 | Low Coolant Level Signal
4 | BRN/GRN | XU600 | Oil Level Signal
5 | RED | A900 | Fused ignition (terminal W)
6 | BLK | F8 | Ground
7-8 | -- | -- | Not Used
9 | BLU/RED | PA600 | Vehicle Speed Signal (oil pressure warning)
10-12 | -- | -- | Not Used
13 | GRN | U5 | Tach Signal (oil pressure warning)
14 | BRN/BLK | XF20 | Seat Belt Switch Signal
15 | BLU/GRN | PU1 | Oil Pressure Switch Signal
16 | GRY/WHT | RM900 | Headlamps ON Signal
17 | GRY/YEL | RB103 | Interior Lamps Dimming Signal
18 | BLU/WHT | PM1 | Generator Input Signal
19 | -- | -- | Not Used
20 | BRN | X70 | Fused Ignition Feed
21 | BRN/PPL | XY2 | ALC Sensor Signal
22 | RED | A16 | Fused Battery Feed
23 | BRN/BLU | XP840 | Security Lamp Signal
24 | BLK | F11 | Lamp Ground
25 | -- | -- | Not Used
26 | BLU/YEL | PB90 | Oil Pressure Sensor Signal

#### Instrument Cluster Connector

Connector Part Information |

• | M 26 - 1

• | 26 Way M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/YEL | XB4 | ABS Input Signal
2 | BRN/YEL | XB105 | Traction Control Input Signal
3 | GRY | R133 | Transmission Malfunction Indicator Signal (1st Design)
4 | BLK/YEL | FB800 | Sport Mode Indicator Signal (1st and 2nd Design) Transmission Malfunction Indicator Signal (2nd Design)
5 | BLK/BLU | FP40 | Fog Lamp Indicator Signal
6 | BLK/WHT | FM13 | LH Turn Signal Indicator
7 | BLK | F2 | Ground
8 | GRY/YEL | RB104 | Interior Lamps Dimming Control
9 | WHT | M75 | High Beam Indicator Control to BCM
10 | BRN/BLU | XP900 | Trunk Lid Open Indicator Control to BCM
11 | RED/BLU | XP808 | Battery Feed Input from DIL Relay
12 | BRN/YEL | XB910 | Headlamps ON Required Indicator Control to BCM
13 | BRN/YEL | XB20 | Airbag Indicator Control to SDM
14 | BRN/BLU | XP23 | MIL Control to ECM
15 | BRN/RED | XA2 | Brake Indicator Signal
16 | BLK/RED | FA825 | Brake To Shift Indicator Control to BCM
17 | BRN/WHT | XM950 | Cruise Indicator Control to ECM
18 | BLK/GRN | FU7 | RH Turn Indicator
19 | BRN | X13 | Fused Ignition Feed
20 | BLU/BLK | PF2 | Fuel Level Signal
21 | BLU | P900 | Coolant Temperature Signal
22 | GRN | U4 | Tach Signal (tach gauge)
23 | BLU/RED | PA6 | Vehicle Speed Signal (speedometer)
24 | BRN/WHT | XM500 | Serial Data (KW 82)
25 | RED | A971 | Fused Battery Feed
26 | BLK | F300 | Controller Ground