For 1990-2009 cars

# 1997 BILL 101 FRENCH LABEL INSTALLATION INSTRUCTIONS

REVISION: 01/19/95

THIS BULLETIN IS BEING REVISED TO OUTLINE CHANGES TO THE USE OF FRENCH LABELS FOR THE 1995 MODEL YEAR AND IS APPLICABLE TO GM OF CANADA ONLY. ---------------------------------------------------------------------- REVISION: 11/06/95

THIS BULLETIN IS BEING REVISED TO OUTLINE CHANGES TO THE USE OF FRENCH LABELS FOR THE 1996 MODEL YEAR AND IS APPLICABLE TO GM OF CANADA ONLY. ---------------------------------------------------------------------- REVISION: 11/14/96

THIS BULLETIN IS BEING REVISED TO OUTLINE CHANGES TO THE USE OF FRENCH LABELS FOR THE 1997 MODEL YEAR AND IS APPLICABLE TO GM OF CANADA ONLY. ---------------------------------------------------------------------- REVISION: 04/01/97

THIS BULLETIN IS BEING REVISED TO OUTLINE CHANGES TO THE USE OF FRENCH LABELS FOR THE 1997 MODEL YEAR AND TO ADD LABEL INFORMATION FOR THE NEW 1997 ISUZU HOMBRE PICK UP TRUCK. THIS BULLETIN IS APPLICABLE TO GM OF CANADA DEALERS ONLY. ----------------------------------------------------------------------

#### SUBJECT: INFORMATION ON 1997 BILL 101 FRENCH LABEL INSTALLATION INSTRUCTIONS

#### MODELS: 1997 PASSENGER CARS AND TRUCKS

ATTACHMENT 1- ALL PASSENGER CARS

* ENGINE COMPARTMENT LABELS (DRWG 52367896, SHEETS 1-4) * PASSENGER COMPARTMENT LABELS (DRWG 52367896, SHEETS 5-8) * TRUNK COMPARTMENT LABELS (DRWG 52367896, SHEETS 9-11)

ATTACHMENT II- DIESEL LABEL INFORMATION FOR BOTH PASSENGER AND LIGHT DUTY TRUCK.

ATTACHMENT III- LIGHT DUTY TRUCK

* ENGINE COMPARTMENT * PASSENGER COMPARTMENT * OTHER

ATTACHMENT IV MEDIUM DUTY TRUCK (C5-6-7, W4-5-7) DRAWING 52367897

ATTACHMENT I

GENERAL- ALL 1997 PASSENGER CARS

LABELS ARE PRESSURE SENSITIVE, THEREFORE, SURFACES MUST BE CLEAN, DRY, WARM AND FREE OF CONTAMINANTS, BEFORE LABELS ARE AFFIXED. LABELS MUST BE PRESSED FIRMLY OVER THEIR ENTIRE SURFACE (BILINGUAL LABELS MAY BE PLACED ON THE TOP OF ENGLISH LABELS).

LOCATE LABELS NEXT TO CORRESPONDING ENGLISH LABELS, UNLESS OTHERWISE NOTED. BOTH LABELS MUST BE READABLE.

#### ENGINE:

1. FAN CAUTION LABEL * IF VEHICLE IS EQUIPPED WITH AN ENGLISH LABEL, PLACE A BILINGUAL LABEL OVER IT. OTHERWISE, PLACE THE FRENCH LABEL ADJACENT TO THE ENGLISH EMBOSSED MESSAGE ON FAN SHROUD.

* FOR SATURN USE 52367175 (FAN & REFRIDGE) * F CAR WARNING PART OF 52368198 * C/H, G CAR WARNING PART OF COMBINED LABEL * FOR SAAB USE 52366361

2. WIPER UPKEEP-DELCO WATER BOTTLE CAP TAG

* FOR ALL APPLICABLE MODELS ADD 52366236 TO THE BACK OF THE ENGLISH TAG WHICH IS PART OF THE BOTTLE ASSEMBLY. (THIS WILL BE USED ON ANY VEHICLE WITH A DELCO SUPPLIED WATER CONTAINER FOR THE WINDSHIELD.)

3. BATTERY CAUTION LABELS

BATTERY LABELS ARE PLACED ON TOP OF THE EXISTING LABEL. USE 52367165 FOR DELCO BATTERIES WITH A SERVICE TAB ON THE RH SIDE OF THE BATTERY. USE 52367166 FOR DELCO BATTERIES WITH A SERVICE TAB ON THE LH SIDE OF THE BATTERY. (THE CUTOUT SHOULD ALLOW THE TAB TO BE LIFTED.)

4. A/C LABEL (R134A)

* ALL VEHICLES USING R134A REFRIGERANT WILL USE THESE 2 LABELS. THEY ARE TO BE PLACED ADJACENT TO THE ENGLISH LABELS IF SPACE PERMITS AND IF NOT THEY ARE TO BE PLACED IN A PROMINENT POSITION SO THAT VIEWERS WILL BE AWARE THE VEHICLE USES R134A REFRIGERANT. THE PART NUMBERS ARE 52366391 AND 52366392.

5. NOTICE THROTTLE BODY ADJUST LABEL (LT1/LT5)

* FOR Y CAR (CORVETTE) PLACE 52365428 ADJACENT TO ENGLISH LABEL PROVIDED.

6. VEHICLE EXHAUST EMISSION

* FOR SAAB USE 52366357

7. HOOD PROP ROD LABEL

* PLACE LABEL 52364164 ADJACENT TO ENGLISH LABEL ON U VAN

8. ENGINE OIL FILL CAP LABEL

* PLACE LABELS 52367565 OR 52357566 (DEPENDING ON WHICH OIL IS USED, SW OR LOW) OVER ENGLISH LABEL ON C,H,K,E,F,J,N,W CARS AND U VAN

9. ACCESSORY BELT ROUTING LABEL

* THE BILINGUAL LABEL SHOULD GO DIRECTLY OVER THE TOP OF THE ENGLISH LABEL SO THAT THE BILINGUAL ONLY SHOWS.

FOR U.S. NO. 10044858 USE 52356837 ON U VAN FOR U.S. NO. 10105211 USE 52361696 ON K,E FOR U.S. NO. 25523397 USE 52354640 ON J,N (LG7) FOR U.S. NO. 10186176 USE 52366054 ON Y (LT1) FOR U.S. NO. 21006214 USE 52363686 ON SATURN FOR U.S. NO. 10114996 USE 52364109 ON W FOR U.S. NO. 10105368 USE 52365429 ON K,E FOR U.S. NO. 10105362 USE 52365519 ON F FOR U.S. NO. 10141993 USE 52365432 ON J,N (LN2) FOR SAAB USE 52366363 USE 52367589 ON SATURN

10. VEHICLE FLUIDS IDENTIFICATION LABEL

* PLACE 52367711 ADJACENT TO EXISTING ENGLISH LABEL ON CADILLAC 4.6L ONLY AND G CAR.

11. A/C REFRIGERANT CHARGING PROCEDURE LABEL

* PLACE LABEL 52366056 ADJACENT TO ENGLISH LABEL ON Y CAR

* PLACE LABEL 52366712 ADJACENT TO ENGLISH LABEL ON C-H CAR.

12. FUSE BLOCK IDENTIFICATION LABEL

* PLACE LABEL 52368327 OVER THE EXISTING ENGLISH LABEL ON CATERA * PLACE LABEL 52363378 OVER THE EXISTING ENGLISH LABEL ON W CAR (QTY-2)

13. CAUTION WIPER LABEL

* PLACE LABEL 52367176 ADJACENT TO THE EXISTING ENGLISH LABEL ON U VAN

14. SPECIAL COOLANT FILL LABEL

* PLACE LABEL 52360259 OVER EXISTING ENGLISH LABEL ON W CAR

15. HDLP BULB REPLACEMENT INST. LABEL

* PLACE LABEL 52356207 ADJACENT TO ENGLISH LABEL ON J AND N CAR

16. INFLATABLE RESTRAINT SYSTEM LABEL

* PLACE LABEL 52367053 ADJACENT TO ENGLISH LABEL ON E, W CARS AND U VAN

17. BRAKE FLUID PRESSURE CAUTION LABEL

* PLACE LABEL 52361684 ADJACENT TO ENGLISH LABEL ON C, H, K, E

18. NOTICE DEXRON III(R) ONLY LABEL

* PLACE 52362564 ADJACENT TO ENGLISH LABEL ON M CAR

19. CAUTION ACTIVE RIDE SUSPENSION LABEL

* PLACE 52362571 ADJACENT TO ENGLISH LABEL ON K, E

20. CAUTION FRONT SUSPENSION GAS UNDER PRESSURE LABEL

* PLACE 52362570 ADJACENT TO ENGLISH LABEL ON K, E

21. CAUTION FUEL FLAMMABLE LABEL

* WRAP FOUR (4) 52362963 LABELS ON ALL VEHICLES AROUND FUEL LINE ADJACENT TO ENGLISH LABEL. IF NO ENGLISH LABEL IS PRESENT, THERE IS NO NEED TO USE THE FRENCH.

22. S.I.R. CAUTION LABELS

* PLACE THREE (3) 52363000 LABELS ON ALL PASSENGER CARS - 1 ON PASSENGER DOOR PILLAR, 1 ON UNDERSIDE OF STEERING COLUMN, 1 ON RADIATOR SUPPORT BAR UNDERHOOD.

23. DEX-COOL(R) (ALL EXCEPT SAAB, M CAR) * PLACE 52368325 ADJACENT TO ENGLISH LABEL ON CATERA, C,H,J,N,G * PLACE 52368212 ADJACENT TO ENGLISH LABEL ON W CAR * PLACE 52368213 ADJACENT TO ENGLISH LABEL ON U VAN

24. HEADLAMP LABEL

* PLACE 52366713 ADJACENT TO ENGLISH LABEL ON G CAR

25. REFRIGERANT CAUTION LABEL

* PLACE 52367382 ADJACENT TO ENGLISH LABEL ON W CAR

26. COMBINED LABEL (ACCESSORY BELT, FAN WARNING, ETC.)

* PLACE 52368198 ADJACENT TO ENGLISH LABEL ON F CAR * PLACE 52366710 ADJACENT TO ENGLISH LABEL ON G, C, H CAR * PLACE 52368308 ADJACENT TO ENGLISH LABEL ON Y CAR

27. CAUTION HIGH VOLTAGE

* PLACE 52366744 (2 PER UNIT) AND 52366747 (1 PER UNIT) ON HEADLAMP ASSEMBLY ADJACENT TO ENGLISH LABELS

28. VEHICLE EXHAUST EMISSION

* PLACE 52366357 ADJACENT TO ENGLISH LABEL ON SAAB. PASSENGER COMPARTMENT

1. SHOCK ABSORBER CAUTION LABEL (4 PER VEHICLE)

* PLACE 52353504 ADJACENT TO ENGLISH LABEL ON K, E CARS

2. ROOF PANEL SPECIAL CARE

* PLACE 52367640 ADJACENT TO ENGLISH LABEL ON Y CAR

3. CAUTION SULFURIC FUMES

* PLACE 52366746 ADJACENT TO ENGLISH LABEL ON G CAR

4. APPLY BRAKE TO SHIFT LABEL

* PLACE 52362974 ON C, H

* PLACE 52366412 ON M

5. ROOF PANEL NOTICE LABEL

* PLACE 52350964 ON LEFT AND RIGHT SIDE ROOF PANELS OVER ENGLISH LABELS ON K, E CARS

6. ANTI THEFT (ON WINDOW LABEL) * PLACE 51368216 ON WINDOW OF CATERA ADJACENT TO ENGLISH LABEL

* PLACE 82368215 ON WINDOW OF C, H CARS ADJACENT TO ENGLISH LABEL * PLACE 52360255 IN GLOVE BOX OF VEHICLE ON F

7. FUSE BLOCK IDENTIFICATION LABELS

* PLACE 52365762 OVER EXISTING LABEL ON F CAR

* PLACE 52366366 OVER EXISTING ENGLISH LABEL ON W

* PLACE 52365763 OVER EXISTING ENGLISH LABEL ON Y

* PLACE LABEL 52355487 OVER EXISTING ENGLISH LABEL ON K, E

* PLACE LABEL 52354729 OVER EXISTING ENGLISH LABEL ON J, N

8. ADJ ASM ACCEL AND CRUISE CONTROL LABEL

* PLACE 52365428 ADJACENT TO ENGLISH LABEL ON Y CAR

9 INTERIOR LIGHT SWITCH TAG

* PLACE LABEL 52363544 ON U VANS

10A CHILDPROOF LOCK LABEL (RR DR WINDOW)

* PLACE 52366354 ADJACENT TO ENGLISH LABEL ON U VAN

* PLACE 52365626 ON EACH REAR DOOR OR WINDOW ON THE PROPER SIDE FOR C,H,K,E,G,W AND SAAB, SATURN, CATERA AND M CAR

10B CHILDPROOF LOCK LABELS (NEAR LK SWITCH) * USE 5236500-2 FOR C, H, G AND SATURN * USE 52368210-11 FOR K, E CARS * USE 52367574-7 FOR W CAR * USE 52363755 (QTY 2) M CAR 11. DUAL MODE RETRACTOR CHILD RESTRAINT SEAT BELT LABEL

* PLACE 52363002 AROUND D-RING SIDE OF BELT DIRECTLY AROUND STITCHED AREA ON U VAN (2 PER JOB) * PLACE 20584675 ON C, H, M (2 PER JOB)

12. ELECTRONIC BRAKE CONTROL INFO TAG

* PLACE LABEL 52363424 ON Y CAR

13. CAUTION-CHILD SEAT BELT WARNING ON LK PILLAR

* PLACE 52367461 ON M, F AND CATERA ON PASSENGER SIDE LOCK PILLAR

14. INFLATABLE RESTRAINT SYSTEM LABEL

* ONLY THE SIR LABEL SHOULD APPEAR ON THE SURFACE OF A S/S, NO OTHER LABELS. * PLEASE NOTE S/S LABELS ARE OFTEN OF VERY STRONG ADHESIVE, CARE SHOULD BE TAKEN THAT THEY ARE APPLIED PROPERLY AS ADJUSTMENT MAY PROVE IMPOSSIBLE. SHOULD SPACE NOT BE AVAILABLE AND THE HEADLINING USED, PLEASE BE SURE THAT THE S/S IN THE UP POSITION COVERS THE LABEL. * FOR CORVETTE USE 52368009 (2) AND 52389100 (1) * FOR SAAB USE 52366359 AND 52366360 * FOR ALL VEHICLES EXCEPT CORVETTE WITH F/FRONTAL USE 52368007 (2) AND 52366758 (1)

15. INSTRUCTION SHEET HUB-CAP INSTALLATION

* PLACE 52360389 IN GLOVE BOX ON C, H

16. ANTI-THEFT LOCKING SYSTEM LABEL

* PLACE 52360256 ADJACENT TO ENGLISH LABEL ON W CAR

17. CAUTION SEAT CODE

* THERE ARE 15 POSSIBLE SEAT LABELS PROVIDED ON A SINGLE SHEET OF BACKING. CARE MUST BE TAKEN TO PUT THE CORRECT LABEL BESIDE THE EXISTING ENGLISH LABEL

18.SEAT OPERATION LABELS

* THERE ARE 5 SEAT OPERATION LABELS WHICH ARE APPLIED TO THE SEAT UPHOLSTERY ON THE U VAN, AS DICTATED BY SEAT TYPE

* USE 52368190-1-2-3-4 AS IS APPLICABLE AND PLACE BESIDE ENGLISH LABEL

19. ROOF LIFT OFF WINDOW STORAGE INSTRUCTIONS (T-ROOF)

* PLACE 52362754 ADJACENT TO ENGLISH LABEL ON F

20. JACK LOCATION LABEL

* PLACE 52362768 ADJACENT TO ENGLISH LABEL ON Y

21.PASS KEY SYSTEM CARD (Y CAR)

* PLACE 52362768 ADJACENT TO ENGLISH LABEL

22. ANTI-LOCK BRAKE LABEL

* PLACE 52365757 ON THE BACK OF THE EXISTING TAG ON U VAN PLACE 52367052 TAG BESIDE EXISTING 2 SIDED TAG

23. TAG ELECTRONIC BRAKE CONTROL INFO

* MAKE SURE TAG 52363424 IS INSTALLED AND GETS TO CUSTOMER ON Y CAR

24. ADJ ASM AND CRUISE CONTROL LABEL

* PLACE 52365428 ADJACENT TO ENGLISH LABEL ON Y

25. SUNROOF SHADE PANEL INSTALLATION CARD

* PLACE 52365760 INSIDE GLOVE BOX ON F

26. NOTICE RADIO DAMAGE

* PLACE LABEL 52366186 ADJACENT TO ENGLISH LABEL ON Y CAR

27. POWER SLIDING DOOR LABEL

* PLACE 52366233 ADJACENT TO ENGLISH LABEL ON U VAN

28. CONVERTIBLE TOP LINER LABEL

* PLACE 52366042 ADJACENT TO ENGLISH LABEL ON CONVERTIBLE F CAR

29. TAG HUMIDITY REMOVAL

* PLACE 52367193 TAG ADJACENT TO ENGLISH TAG ON M CAR

30. EXTENDED MOBILITY TIRE LABEL

* PLACE 52366231 ADJACENT TO EXISTING ENGLISH ON Y CAR

31. SEAT BELT SIR INFORMATION

* PLACE 52367461 ON M CAR PASSENGER SIDE LOCK PILLAR

TRUNK

1. TEMPORARY SPARE LABEL

* PLACE 52366362 ADJACENT TO EXISTING ENGLISH LABEL ON SAAB

2. SPARE WHEEL RETENTION LABEL

* PLACE 52366043 ADJACENT TO ENGLISH LABEL ON U VAN

3. JACK LOCATOR LABEL

* PLACE 52362568 ON M

4. WIRE WHEEL COVER LOCK REMOVAL LABEL

* PLACE 52353419 ON C, H CAR

* PLACE 52361679 ON W (ALUM. SIMUL.)

5. NOTICE-CLEAN OFF FUEL PROMPTLY

* PLACE 52367462 ADJACENT TO ENGLISH LABEL ON B, W CARS

6. INFLATION CANISTER LABEL

* PLACE 746415 ON F

7. SPACE SAVER SPARE TIRE LABEL

* PLACE 52350966 ON RIM NEXT TO ORIGINAL LABEL AFTER REMOVING TIRE AND INFLATION CANISTER ON F CAR

8. JACK ASSEMBLY CAUTION LABEL

* PLACE 52367590 ADJACENT TO ENGLISH LABEL ON ALL CARS EXCEPT SAAB, SATURN, AND M * PLACE 52367566 ADJACENT TO ENGLISH LABEL ON M CAR

9. JACK INSTRUCTION LABELS

* PLACE 52361492 ADJACENT TO ENGLISH LABEL ON C, H (BUICK, OLDS, PONTIAC) * PLACE 52366905 ON F CAR * PLACE 52367977 ON U * PLACE 52362563 ON M * PLACE 52366252 ADJACENT TO ENGLISH LABEL ON W * PLACE 52367172 ON Y CAR * PLACE 52368310 ON CATERA * PLACE 52368203 ON E,K * PLACE 52364449 ON J,N * PLACE 52364450 ON J * ADD 52365012 ON SATURN * ADD 52366358 ON SAAB * ADD 52366743-A AND 52366743 B TO TRUNK FILLER PANEL BOARD ON G

10. REMOTE LOCKING FUEL DOOR LABEL

* PLACE 52351460 ON BUMPER FILLER PANEL ADJACENT TO ENGLISH LABEL ON K, E CARS

11 TRACTION CONTROL (ON SPARE)

* PLACE LABEL 52367572 ON F CAR

12. NOTICE CONVERTIBLE TOP CLOSE LABEL

* PLACE LABEL 52362930 ON F CARS

13. CENTER HUB CAP REMOVAL INSTRUCTION

* PLACE 52354730 ADJACENT TO ENGLISH LABEL ON J, N CARS

14. TRAILER TOWING NOTICE LABEL

* PLACE 52355167 ADJACENT TO ENGLISH LABEL ON K, E

15. AMCOR SECURITY LUG NUTS

* PLACE 52362957 ON J, N, W (PONTIAC ONLY)

16. CONVENIENCE NET LABEL

* PLACE 52365608 ADJACENT TO ENGLISH LABEL ON U VAN

17. INFLATOR OPERATOR INSTRUCTIONS

* PLACE 52381963 ADJACENT TO ENGLISH LABEL

18. TIRE PRESSURE SENSOR FRONT WHEEL AND REAR WHEEL

* ADD 52363705 (FRT) QTY 2 ON Y CAR * ADD 52363706 (RR) QTY 2 ON Y CAR

19. REMOVE AND DISCARD ALL EXTRANEOUS ENGLISH ADVERTISING.

LABELS WHICH ARE RELEASED LATE WILL BE ADDED TO THIS ATTACHMENT WHEN THE INSTALLATION INSTRUCTIONS ARE REISSUED.

ATTACHMENT II

DIESEL LABEL INFORMATION FOR L.D. TRUCK

#### GENERAL INFORMATION:

LABELS ARE PRESSURE SENSITIVE; THEREFORE, SURFACES MUST BE CLEAN, DRY, WARM AND FREE OF CONTAMINANTS, BEFORE LABELS ARE AFFIXED. LABELS MUST BE PRESSED FIRMLY OVER THEIR ENTIRE SURFACE.

LOCATE LABELS NEXT TO ENGLISH LABELS, UNLESS OTHERWISE NOTED. BOTH LABELS SHOULD BE READABLE.

#### ENGINE COMPARTMENT:

1. MAXIMUM VOLTAGE CAUTION LABEL

* PLACE 52354639 ADJACENT TO ENGLISH LABEL

2. OIL FILLER CAP LABEL

* PLACE LABEL 52367565, 52357566 OVER ONE OF THE ORIGINAL LABELS ON THE OIL FILLER CAP. (KEY ON OIL REQUIRED)

3. DIESEL SERVICE 6.5L

* PLACE 52364127 ADJACENT TO 10149667

PASSENGER COMPARTMENT

1. DIESEL ENGINE START PROCEDURE LABEL

* PLACE 52367143 ADJACENT TO ENGLISH LABEL

ATTACHMENT III

GENERAL-C/K, P, S/T TRUCK, AND G AND M VANS, RODEO, TROOPER, HOMBRE

LABELS ARE PRESSURE SENSITIVE; THEREFORE, SURFACES MUST BE CLEAN, DRY, WARM AND FREE OF CONTAMINANTS, BEFORE LABELS ARE AFFIXED. LABELS MUST BE PRESSED FIRMLY OVER THEIR ENTIRE SURFACE.

LOCATE LABELS NEXT TO CORRESPONDING ENGLISH LABELS, UNLESS OTHERWISE NOTED. BOTH LABELS MUST BE READABLE.

ENGINE

1. FAN CAUTION LABEL

* PLACE 52362522 AND 52362525 ADJACENT TO ENGLISH LABEL ON TRACKER/SUNRUNNER * PLACE 52366044 ADJACENT TO ENGLISH LABEL ON P TRUCK

2. BATTERY CAUTION LABELS

* USE 52367165 FOR BATTERIES WITH RH SERVICE TAB AND 52367166 FOR BATTERIES WITH LH SERVICE TAB * THE SERVICE/WARRANTY TAB IS NOT TO BE COVERED BY THE BILINGUAL PLACED ON TOP OF THE ENGLISH LABEL

3. BATTERY CHARGE INDICATOR LABEL

* PLACE 52362523 ON TRACKER/SUNRUNNER

4. AIR CONDITIONER LABELS

* FOR ALL R134A VEHICLES PLACE 52366391 AND 52366392 LABELS ADJACENT TO EXISTING ENGLISH LABELS

5. HOOD PROP ROD LABEL

* PLACE LABEL 52354520 OVER ORIGINAL ENGLISH LABEL ON M VAN, L VAN

6. ENGINE OIL FILL CAP LABEL

* PLACE LABEL 52367565, 52367566 OVER ORIGINAL ENGLISH LABEL ON THE OIL FILL CAP. (KEY ON TYPE OF OIL REQUIRED) ON P TRUCK, S/T TRUCK, C/K TRUCK, HOMBRE

7. ACCESSORY BELT ROUTING LABEL

* USE 52360932 IN PLACE OF 10085701 ON P, S/T, C/K TRUCK, HOMBRE * USE 52361584 IN PLACE OF 10085749 ON P TRUCK, C/K TRUCK * USE 52356184 IN PLACE OF 10044337 ON M VAN, L VAN, S/T TRUCK, HOMBRE * USE 52362146 IN PLACE OF 10129531 ON M VAN, L VAN * USE 52362145 IN PLACE OF 10129530 ON M VAN, L VAN * USE 52360631 IN PLACE OF 10100080 ON S/T TRUCK, HOMBRE * USE 52363443 IN PLACE OF 10129592 ON L, M VAN

PLACE BILINGUAL LABEL OVER EXISTING ENGLISH LABEL. (IF LABEL IS FRENCH LANGUAGE ONLY, PLACE ADJACENT TO ENGLISH LABEL.)

* USE 52367119 ON BLANK AREA OF 10141993 ON S/T TRUCK AND HOMBRE (2.2L) SO THAT BOTH LANGUAGES SHOW 8. RADIATOR CAUTION LABEL

* PLACE 52356339 OVER EXISTING ENGLISH LABEL (RODEO AND TROOPER TRUCKS)

9. CAUTION HOT SURFACE LABEL

* PLACE 52361669 DIRECTLY ON TOP OF ENGLISH LABEL ON S/T TRUCK, HOMBRE

10. BATTERY AND CABLE INSTALLATION LABEL

* PLACE 52362147 ADJACENT TO ENGLISH LABEL ON S/T TRUCK, HOMBRE

11. CAUTION FUEL FLAMMABLE LABEL (4 PER VEHICLE)-ISUZU PRODUCTS ONLY

* PLACE 52362963 AROUND FUEL LINE ADJACENT TO ENGLISH LABELS. IF NO LABELS PRESENT, DO NOT USE LABELS. APPLIES TO TRACKER- SUNRUNNER, RODEO AND TROOPER TRUCK

12. ENGINE JUMP START LABEL

* PLACE 52364147 ADJACENT TO ENGLISH LABEL ON L, M VAN

13. INFLATABLE RESTRAINT SYSTEM

* PLACE 52367053 ADJACENT TO ENGLISH LABEL ON L, M VAN, C/K, S/T, RODEO, TROOPER, HOMBRE

* PLACE 52367053 ADJACENT TO ENGLISH LABEL ON C/K TRUCK

14. REFRIGERANT CAUTION LABEL

* PLACE 52356341 ADJACENT TO ENGLISH LABEL ON TROOPER

* PLACE 52362521 ADJACENT TO ENGLISH LABEL ON TRACKER/SUNRUNNER

* PLACE 52362524 ADJACENT TO ENGLISH LABEL ON TRACKER/SUNRUNNER

15. SIR CAUTION LABELS (1 UNDERHOOD, 2 INSIDE TRUCK)

* PLACE 1 LABEL ON RADIATOR SUPPORT, 1 LABEL ON UNDERSIDE OF STEERING COLUMN, AND 1 LABEL ON THE PASSENGER SIDE DOOR FRAME ON ALL JOBS WITH SIR * ALL EXCEPT P TRUCK

16 DEX COOL(R)

* PLACE 52368326 ADJACENT TO ENGLISH LABEL ON P,G,L,M,S/T,C/K TRUCKS AND HOMBRE

ATTACHMENT III

PASSENGER COMPARTMENT

1. TAG HUMIDITY REMOVAL

* PLACE 52366346 ON BACK OF EXISTING TAG FOR TRACKER/SUNRUNNER

2. SHOCK ABSORBER CAUTION LABEL

* PLACE 52353504 ADJACENT TO THE ENGLISH LABELS ON THE SHAFTS OF EACH SHOCK ABSORBER BY RAISING THE VEHICLE ON A HOIST ON S/T TRUCK AND HOMBRE (4 LABELS)

3. TRANSFER CASE SHIFT LABEL

* PLACE 52352672 ON LH SUNVISOR IN DOWN POSITION AND LOCATE LABEL IN CENTRE OF SUNVISOR ON: S/T TRUCK, OMBRE

4. FUSE BLOCK IDENTIFICATION (C/K TRUCK)

* PLACE 52367387 OVER EXISTING ENGLISH LABEL

5. ENGINE START PROCEDURE LABEL

* PLACE 52364159 ADJACENT TO ENGLISH LABEL ON G VAN (L19) C/K TRUCK (L19) * PLACE 52363700 ADJACENT TO ENGLISH LABEL ON P TRUCK

6. ENGINE COVER REMOVAL LABEL

* PLACE LABEL 52354517 OVER EXISTING ENGLISH LABEL IN GLOVE COMPARTMENT AREA ON M VAN AND L VAN

7. CHILDPROOF LOCK LABEL

* PLACE 52362462 ADJACENT TO ENGLISH LABEL ON TROOPER TRUCK

* PLACE 52367466-67 ON RR DR LK PLRS

8. UTILITY VEHICLE HANDLING

* PLACE LABEL 52354648 ADJACENT TO EXISTING ENGLISH LABEL ON C/K TRUCK, S/T TRUCK, TROOPER, RODEO, HOMBRE

9. DUAL MODE RETRACTOR CHILD RESTRAINT SEAT BELT LABEL

* PLACE 20584675 AROUND BELT AT STITCHING ON S/T TRUCK, HOMBRE, TRACKER (2 PER JOB)

10. 4 X 4 TRANSFER CASE INFORMATION LABEL

* PLACE 52355163 ADJACENT TO ENGLISH LABEL ON S/T TRUCK

11. COMMERCIAL TRAILERING LABEL

* PLACE LABEL 52355329, 52355330 OR 52355331 ADJACENT TO ENGLISH LABEL WITH CORRESPONDING WEIGHT ON P TRUCK

12. UNLEADED FUEL DASH LABEL

* PLACE 52356603 ON TOP OF ENGLISH LABEL ON TROOPER TRUCK

13. CENTER A/RST CAUTION LABEL (C/K TRUCK)

* PLACE 52367390 ADJACENT TO EXISTING ENGLISH LABEL

14. SI ACCESS PANEL (S/T TRUCK, HOMBRE)

* PLACE 52367460 ADJACENT TO EXISTING ENGLISH LABEL

15. ANTI-LOCK BRAKE SYSTEM

* PLACE 52362999 ON THE BACK OF EXISTING ANTI-LOCK BRAKE TAG FOR M VAN, L VAN, S/T TRUCK, HOMBRE

16. ELECTRICAL GROUND STRAP LABEL

* PLACE 52362148 ADJACENT TO ENGLISH LABEL ON P TRUCK

17. CAUTION WASHER SOLVENT LABEL

* PLACE 52362752 ON REAR WASHER CONTAINER ON TROOPER

18. UTILITY VEHICLE ALL WHEEL DRIVE OR 4 W/D INSTRUCTION

* PLACE 52364152 ADJACENT TO ENGLISH LABEL

19. PARK BRAKE OPER. INST

* PLACE 52363416 ADJACENT TO 15638160 ON G VAN

20. ADJUSTABLE SAFETY BOLT ANCHOR

* PLACE 52365062 ADJACENT TO ENGLISH LABEL ON L, M VAN QTY 2

21. S.I.R. SYSTEM (ON S/S)

* PLACE 52365754 (DRIVER SIDE) ADJACENT TO ENGLISH LABEL ON C/K FOR S/T AND HOMBRE USE 52366758 * FOR TROOPER, RODEO, G, L, M USE 52368007

22. APPLY BRAKE TO SHIFT

* PLACE 52366412 ADJACENT TO EXISTING ENGLISH LABEL (TRACKER, SUNRUNNER, TROOPER, RODEO)

23 INFLATABLE RESTRAINT (ON SIS) SUSP OPTION ONLY

* PLACE 52367469 ON C/K TRUCK ONLY WHEN SUSP' IS AVAILABLE . 24 LKG PIN STORAGE (SEATS) . * PLACE 52368214 ADJACENT TO ENGLISH LABEL . 25. SEAT BELT TENSION PRODUCTION . * PLACE 52366108 ADJACENT TO EXISTING LABEL ON C/K TRUCK . 26. AUTO OVERDRIVE NOTICE (TRAILERING, TOWING)

* PLACE 52366355 ADJACENT TO ENGLISH LABEL ON C/K TRUCK

27. SHOULDER BELT ADJUST FEATURE LABEL

* PLACE 52366715 ADJACENT TO ENGLISH LABEL FOR C/K TRUCK

28. INT & RR SI DOOR CHECK STRAP LABEL

* PLACE 52366199 ADJACENT TO EXISTING ENGLISH LABEL ON G VAN

29. R/SEAT BELT & SEAT LATCH CAUTION

* PLACE 52367972 ADJACENT TO EXISTING ENGLISH LABEL ON G VAN

TRUNK/INTERIOR/STORAGE AREAS

1. JACK ASSEMBLY CAUTION LABEL

* PLACE 52367590 ADJACENT TO EXISTING ENGLISH LABEL ON ALL JOBS EXCEPT ISUZU PRODUCTS * PLACE 52362520 ON OPPOSITE SIDE TO ENGLISH LABEL ON JACK ASSEMBLY ON TRACKER

2. JACK INSTRUCTION LABEL

* PLACE 52362825 ON OPPOSITE SIDE TO ENGLISH ON P TRUCK * PLACE 52368195 ON OPPOSITE SIDE TO ENGLISH ON G VAN * PLACE 52367171 ON OPPOSITE SIDE TO ENGLISH ON M/L VAN * PLACE 52352519 ON OPPOSITE SIDE TO ENGLISH ON TRACKER

THE FOLLOWING ARE ALL 2 SIDED TAGS. CARE MUST BE USED TO PICK THE LABEL WHICH MEETS THE PHYSICAL CONDITIONS OF THE TRUCK (MODEL OPTION SERIES ETC.). THESE LABELS ARE TO BE STORED WITH THE ENGLISH LABELS BY THE JACK.

S/T TRUCK, HOMBRE C/K TRUCK 52367210 (06-16) 52366249 (06-16) 52367211 (03-43-53) 52366250 (310,314,03) 52366253 (300,43) 52366254 (2-300, 03-53)

3. LIGHT SUPPORT CAUTION LABEL

* PLACE 52362144 ADJACENT TO ENGLISH LABEL ON S/T TRUCK, HOMBRE (3 PER VEHICLE)

4. TAILGATE OPENING LABEL

* PLACE 52356599 ADJACENT TO EXISTING LABEL ON TROOPER

5. CAUTION FUEL SPRAY LABEL

* PLACE 52362319 ADJACENT TO ENGLISH LABEL ON P TRUCK

6. REAR DOOR CHECK STRAP LABEL

* PLACE 52363735 ADJACENT TO ENGLISH LABEL (C/K SUBURBAN)

* PLACE 52367713 ADJACENT TO ENGLISH LABEL ON C/K, SUBURBAN, G VAN

7. OUTSIDE SPARE TIRE RELEASE LEVER

* PLACE 52364153 ADJACENT TO ENGLISH LABEL ON RODEO

ATTACHMENT IV

GENERAL-MD TRUCK (1997) C5-6-7, W4-F6-7

LABELS ARE PRESSURE SENSITIVE; THEREFORE, SURFACES MUST BE CLEAN, DRY, WARM, AND FREE OF CONTAMINANTS, BEFORE LABELS ARE AFFIXED. LABELS MUST BE PRESSED FIRMLY OVER THEIR ENTIRE SURFACE.

LOCATE LABELS NEXT TO ENGLISH LABELS, UNLESS OTHERWISE NOTED. BOTH LABELS SHOULD BE READABLE.

ENGINE COMPARTMENT

1. BATTERY

* PLACE BILINGUAL BATTERY LABELS OVER EXISTING LABELS AS INDICATED: 52363361 OVER 1981730 52366360 OVER 1981734 52363362 OVER 1981735 52363367 OVER 1981736 52363359 OVER 1981733

2. FAN BLADES

* PLACE 52364320 OVER EXISTING ENGLISH ONLY LABEL ON W TRUCKS

3. CAUTION - NEVER OPEN HOT (ON SURGE TANK TOP)

* PLACE 52364362 OVER EXISTING ENGLISH ONLY LABEL ON W TRUCKS

4. ETHER START NOTICE LABEL

* PLACE 52363056 ADJACENT TO ENGLISH LABEL ON C5-6-7 TRUCK

5. NOTICE ENGINE START FLUIDS

* PLACE 52364315 OVER EXISTING ENGLISH ONLY LABEL ON W TRUCKS

6. CLUTCH CAUTION TAG (ON BELL HOUSING)

* PLACE 52367980 ADJACENT TO ENGLISH ONLY LABEL

7. NOTICE REPLACE AIR FILTER ELEMENT (W4-5-7)

* PLACE 52364363 ADJACENT TO EXISTING ENGLISH LABEL

8. NOTICE USE DOT 3 ONLY (W4)

* PLACE 52364357 OVER EXISTING ENGLISH LABEL

9. BATTERY TRAY REMOVAL

* PLACE 52366748 ADJACENT TO 15987018

10. A/C LABELS

* PLACE 52366391,52366392 ADJACENT TO ENGLISH LABELS AS REQUIRED FOR C5-6-7-W4 * PLACE 52367986 ADJACENT TO ENGLISH LABELS AS REQUIRED FOR F6-7

PASSENGER COMPARTMENT

1. DIESEL START FLUID WARNING LABEL (C5-6-7)

* PLACE 52363052 ADJACENT TO ENGLISH LABEL ON S/S

2. DIESEL ENGINE START PROCEDURE (C5-6-7)

* PLACE 52367143 ADJACENT TO ENGLISH LABEL ON S/S (LABEL UNIQUE TO CANADA DUE TO FUEL)

3. DAYTIME RUNNING LIGHTS (C5-6-7)

* PLACE 52362143 OVER EXISTING ENGLISH ONLY LABEL

4. 2-SPEED REAR AXLE SHIFT LABEL (C5-6-7)

* PLACE 52363112 ADJACENT TO EXISTING ENGLISH LABEL 2011705

5. ROOF VENT INST. (W4)

* PLACE 52364317 ADJACENT TO EXISTING ENGLISH LABEL (ON VENT)

6. REAR AXLE OPERATIONS LABEL (C5-6-7)

* PLACE 52363054 ADJACENT TO EXISTING ENGLISH LABEL 15504240

7. ENGINE START PROCEDURE

* PLACE 52364354 (W4) ADJACENT TO ENGLISH LABEL

8. NOTICE PARK BRAKE

* PLACE 52364319 ADJACENT TO EXISTING ENGLISH LABEL

9. TRANSMISSION SHIFT INST. LABELS (C5-6-7 TRUCKS)

* PLACE 52363057 ADJACENT TO 20181231 * PLACE 52363059 ADJACENT TO 703199 * PLACE 52363050 ADJACENT TO 15504169 * PLACE 52363053 ADJACENT TO 716500 * PLACE 52363113 ADJACENT TO 703198 * PLACE 52363055 ADJACENT TO 15630600 * PLACE 52366106 ADJACENT TO 15963551 * PLACE 52366107 ADJACENT TO 15668196 * PLACE 52367978 ADJACENT TO 15739200

OTHER LOCATIONS (OUTSIDE SURFACE, FRAME RAILS, ETC.)

1. NOTICE WATER SEPARATOR (W4)

* PLACE 52364358 ADJACENT TO EXISTING ENGLISH ONLY LABEL

2. NOTICE TRANSMISSION FLUID (W4)

* PLACE 52364321 OVER TOP OF EXISTING ENGLISH ONLY LABEL

3. CAUTION TILT CAB (REAR DOOR OF CAB O/S LEFT SIDE) (W4)

* PLACE 52366827 OVER EXISTING ENGLISH LABEL * PLACE 52367975 OVER EXISTING ENGLISH LABEL ON F6-7

4. CAUTION TILT CAB (W4)

* PLACE 52364356 ADJACENT TO EXISTING ENGLISH LABEL * PLACE 52367974 ADJACENT TO EXISTING ENGLISH LABEL ON F6-7

5. LOCK (ON CAB SUPT) (W4)

* PLACE 52364318 OVER EXISTING ENGLISH LABEL

6. AVOID DRILLING LABEL (ON FRAME RAIL) (C5-6-7)

* PLACE 52362153 OVER EXISTING ENGLISH LABEL

7. CAUTION AUXILIARY START SWITCH (REAR OF CAB O/S)

* PLACE 52364316 ADJACENT TO EXISTING ENGLISH LABEL

8. FUEL MISER LABEL (C5-6-7)

* PLACE 52367383 ADJACENT TO EXISTING ENGLISH LABEL.

9. RAD FILL NOTICE (DIESEL CATERPILLAR COOLANT LABEL C-5-6-7)

* PLACE 52367391 ADJACENT TO EXISTING ENGLISH LABEL.

10 ETHER NOTICE LABEL

* PLACE 52368199 ADJACENT TO EXISTING ENGLISH LABEL

11 SYNTHETIC LUBE LABEL (F6-7)

* PLACE 52367979 ADJACENT TO ENGLISH LABEL

12 NOTICE ELECTRIC BOX CONNECTOR LABEL (F6-7)

* PLACE 52367981 ADJACENT TO ENGLISH LABEL

13 CAUTION MOVING PARTS LABEL

* PLACE 52367982 ADJACENT TO ENGLISH LABEL

14 CAUTION WIPER CAN CYCLE LABEL (F6-7)

* PLACE 52367983 ADJACENT TO ENGLISH LABEL

15 NO STEP LABEL (F6-7)

* PLACE 52367984 DIRECTLY OVER EXISTING LABEL

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.