For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the front seatback. Refer to Front Seat Back Replacement .
3. Remove the retaining rings from the front seat cushion cover.
4. Remove the front seat cushion cover.
5. Unroute the heating element wiring from the seat cushion pad.

### Installation Procedure

1. Route the heating element wiring through the seat cushion pad.
2. Install the front seat cushion cover.
3. Install the retaining rings to the front seat cushion cover.
4. Install the front seatback. Refer to Front Seat Back Replacement .
5. Install the front seat. Refer to Seat Replacement .