For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the outer finish panel from the front seat cushion. Refer to Seat Cushion Outer Trim Panel Replacement .
3. Disconnect the electrical connectors from the seat adjuster control switch.

The wiring harness is routed under the front seat cushion frame and is secured by tie downs.

4. Remove the seat adjuster control switch.

### Installation Procedure

1. Install the seat adjuster control switch.
2. Connect the electrical connectors to the seat adjuster control switch.
3. The wiring harness is routed under the front seat cushion frame. Secure the wiring harness to the seat frame with tie straps in order to prevent damaging.
4. Install the outer finish panel to the front seat cushion. Refer to Seat Cushion Outer Trim Panel Replacement .
5. Install the front seat. Refer to Seat Replacement .