For 1990-2009 cars

Caution: Avoid taking the following actions when you service wheel brake parts:

• | Do not grind brake linings.

• | Do not sand brake linings.

• | Do not clean wheel brake parts with a dry brush or with compressed air.

Some models or aftermarket brake parts may contain asbestos fibers which can become airborne in dust. Breathing dust with asbestos fibers may cause serious bodily harm. Use a water-dampened cloth in order to remove any dust on brake parts. Equipment is available commercially in order to perform this washing function. These wet methods prevent fibers from becoming airborne.