For 1990-2009 cars

### Tools Required

• | J 8001 Dial Indicator Set

• | J 25022 Front End Play Checking Adapter

• | J 24773-A Oil Pump Remover

1. Install J 25022 and J 24773-A onto the turbine shaft.
2. Attach J 8001 rod to the converter housing using one of the bolt holes.
3. Mount Dial Indicator J 8001 on the rod and index it to the turbine shaft.
4. Apply upward pressure by lifting on J 25022 until resistance is met and set the dial indicator to 0.

Important: If the end play is not correct, repeat the adapter case selective washer procedure.

5. Lift the turbine shaft further upwards with J 25022 . The end play should measure 0.1 to 0.8 mm (0.004 to 0.03 in).
6. Remove the tools.