For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the front seatback. Refer to Front Seat Back Replacement .
3. Remove the front seat cushion cover retaining rings.
4. Remove the front seat cushion cover.
5. Unroute the seat cushion heating element wiring from seat cushion pad.

### Installation Procedure

1. Route the seat cushion heating element wiring through the seat cushion pad.
2. Install the front seat cushion cover.
3. Install the front seat cushion cover retaining rings.
4. Install the front seatback. Refer to Front Seat Back Replacement .
5. Install the front seat. Refer to Seat Replacement .