For 1990-2009 cars

In event of a power failure, the sunroof panel may be opened or closed by using the special tool (screwdriver) that has been provided in the tool kit in the rear compartment (with the jack). There is a cover on the rear of the overhead console (center), which is easily removed. This will allow manual cranking of the motor and drive gear. After each interruption of power, the motor must be reprogrammed.