For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement
2. Remove trim panel retaining block. Refer to Rear Side Door Trim Panel Bracket Replacement
3. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement
4. Remove the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement
5. Remove the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement
6. Remove the door lower weatherstrip. Refer to Rear Side Door Bottom Auxiliary Sealing Strip Replacement
7. Remove the door vent window and division channel. Refer to Rear Side Door Stationary Window and Front Channel Replacement
8. Remove the door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement
9. Remove the door window up stop. Refer to Rear Side Door Window Stop Bumper Replacement
10. Remove the door window regulator and motor. Refer to Rear Side Door Window Regulator Replacement
11. Remove the door window. Refer to Rear Side Door Window Replacement
12. Remove the door upper sealing strip. Refer to Rear Door Upper Sealing Strip Replacement
13. Remove the speaker. Refer to Speaker Replacement in Entertainment.
14. Remove the inside door handle. Refer to Rear Side Door Inside Handle Replacement
15. Remove the door lock. Refer to Rear Door Lock Replacement
16. Remove the door outside handle. Refer to Rear Side Door Outside Handle Replacement
17. Remove the side door molding. Refer to Door Body Side Molding Replacement in Exterior Trim.
18. Remove the door check link. Refer to Rear Side Door Check Link Replacement
19. Remove the door rubber conduit. Refer to Rear Side Door Conduit Replacement
20. Remove the door. Refer to Rear Side Door Removal

### Installation Procedure

1. Install the door. Refer to Rear Side Door Removal
2. Install the door rubber conduit. Refer to Rear Side Door Conduit Replacement
3. Install the door check link. Refer to Rear Side Door Check Link Replacement
4. Install the side door molding. Refer to Door Body Side Molding Replacement in Exterior Trim.
5. Install the door window. Refer to Rear Side Door Window Replacement
6. Install the door outside handle. Refer to Rear Side Door Outside Handle Replacement
7. Install the door lock. Refer to Rear Door Lock Replacement
8. Install the inside door handle. Refer to Rear Side Door Inside Handle Replacement
9. Install the speaker. Refer to Speaker Replacement in Entertainment.
10. Install the door upper sealing strip. Refer to Rear Door Upper Sealing Strip Replacement
11. Install the door window. Refer to Rear Side Door Window Replacement
12. Install the door window regulator and motor. Refer to Rear Side Door Window Regulator Replacement
13. Install the door window up stop. Refer to Rear Side Door Window Stop Bumper Replacement
14. Install the door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement
15. Install the door lower weatherstrip. Refer to Rear Side Door Bottom Auxiliary Sealing Strip Replacement
16. Install the door vent window division channel. Refer to Rear Side Door Stationary Window and Front Channel Replacement
17. Install the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement
18. Install the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement
19. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement
20. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement