For 1990-2009 cars

### Disassembly Procedure

1. Remove the propeller shaft. Refer to Two-Piece Propeller Shaft Replacement .
2. Support the insulator (2) on a vice.
3. Using a suitable tool, press the bearing (3) out of the insulator (2).
4. Discard the bearing, it is not reusable and must be replaced.

### Assembly Procedure

#### Tools Required

J 21474-20 Control Arm Bushing Driver

1. Using the J 21474-20 , press the bearing (1) into the insulator (2).
2. Install the propeller shaft. Refer to Two-Piece Propeller Shaft Replacement .