For 1990-2009 cars

### Removal Procedure

1. Lift the covers that conceal the screws (one at each end) in order to remove the front assist handle.
2. Remove the screws from the front assist handle.
3. Remove the front assist handle.

### Installation Procedure

1. Install the front assist handle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws to the front assist handle.

Tighten
Tighten the front assist handle screw to 1.5 N·m (13 lb in).

3. Close the front assist handle covers that conceal the screws (one at each end).