For 1990-2009 cars

#### Cellular Telephone (Base System)

Connector Part Information |

• | ZM 9-3

• | 9 Way M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X410 | B+ from Fuse #14
2 | BLK | F410 | Ground to G201
3 | BRN/WHT | XM161 | Serial Data (Class 2)
4 | RED | A411 | B+ from Multifunction Relay K134
5 | WHT | M16 | Cell Phone Negative Output
6 | BRN/WHT | XM16 | Cell Phone Positive Output
7-9 |  |  | Not Used

#### Cellular Telephone (Bose System)

Connector Part Information |

• | ZM 9-3

• | 9 Way M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X10 | B+ from Fuse #14
2 | BLK | F10 | Ground to G201
3 | BRN/WHT | XM15 | Serial Data (Class 2)
4 | RED | A11 | B+ from Multifunction Relay K134
5 | WHT | M16 | Cell Phone Negative Output
6 | BRN/WHT | XM16 | Cell Phone Positive Output
7-9 |  |  | Not Used

#### Compact Disk Changer (Base System)

Connector Part Information |

• | ZF 9-21

• | 9 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F10 | CD Common
2 | WHT | M17 | LH CD Output Signal
3 | BLU | P15 | RH CD Output Signal
4 |  | S2 | Shield Wire
5 | RED | A211 | B+ from Fuse #8
6 | BLK | F111 | Ground to G201
7 | YEL | B220 | CD Data Bus
8-9 |  |  | Not Used

#### Compact Disk Changer (Bose System)

Connector Part Information |

• | 12047531

• | ASM 10F M/P 100 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WHT | M45 | LH CD Output Signal
2 | BLU | P45 | RH CD Output Signal
3 | BLK | F45 | CD Common
4 |  | S5 | Shield Wire
5 | RED | A201 | B+ from Fuse #8
6 | -- | -- | Not Used
7 | BLK | F101 | Ground to G201
8-9 | -- | -- | Not Used
10 | B20 | YEL | CD Data Bus

#### Heated Outside Rear View Mirror and Rear Window Defogger Relay K35

Connector Part Information |

• | ZF 6-14

• | 6 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X84 | B+ from Fuse #14
2 | RED | A18 | B+ from Fuse #34
3 | -- | -- | Not Used
4 | BLK/WHT | FM14 | Defogger Switch Input
5 | BLK/WHT | FM10 | Heated Mirrors On Signal
6 | BLK | F84 | Ground to G103
7 | -- | -- | Not Used
8 | BRN | X15 | Rear Defogger On Signal

#### Inflatable Restraint Steering Wheel Module Coil

Connector Part Information |

• | ZF 8-5

• | 8 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F122 | Ground to G201
2 | BRN/WHT | XM1 | Horn Relay Control Signal
3 | RED/WHT | AM116 | LED Control Signal
4 | BLU/RED | PA101 | Steering Wheel Switch Signal
5-6 | -- | -- | Not Used
7 | YEL/WHT | BM 30 | Driver Front Airbag High Signal
8 | YEL | B30 | Driver Front Airbag Low Signal

#### Radio, AM/FM Stereo and Clock and Tape Player and Compact Disk Player (Base System)

Connector Part Information |

• | 12110115

• | ASM 32F M/P 100 (DK BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
E1 | YEL | B220 | CD Data Bus
E2-E4 | -- | -- | Not Used
E5 | GRY/YEL | RB40 | Illumination Signal
E6 | -- | -- | Not Used
E7 | WHT | M16 | Cellular Phone Negative Input
E8 | BRN/WHT | XM16 | Cellular Phone Positive Input
E9 | -- | -- | Not Used
E10 | BLK | F10 | CD Common
E11 | WHT | M17 | LH CD Input Signal
E12 | GRN | U41 | LH Rear Positive Output
E13 | BRN/GRN | XU42 | LH Rear Negative Output
E14 | BRN/YEL | XB10 | RH Front Negative Output
E15 | YEL | B8 | RH Front Positive Output
E16 | BLK | F40 F49 | Ground to G201
F1 | RED | A52 | B+ from Multifunction Relay K134
F2 | -- | -- | Not Used
F3 | RED/WHT | AM110 AM116 | Radio ON Signal Output
F4 | GRY/GRN | RU72 | B+ from Fuse #26
F5 | BLK | F49 | Ground to G201
F6 | BRN/WHT | XM830 | Serial Data (Class 2)
F7 | -- | -- | Not Used
F8 | BLU/RED | PA101 | Steering Wheel Switch Input
F9 | BLK | B899 | Ground to G201
F10 | -- | -- | Not Used
F11 | BLU | P15 | RH CD Input Signal
F12 | BLU | P1 | LH Front Positive Output
F13 | BRN/BLU | XP4 | LH Front Negative Output
F14 | BRN/WHT | XM42 | RH Rear Negative Output
F15 | WHT | M42 | RH Rear Positive Output
F16 | -- | -- | Not Used

#### Radio, Antenna Amplifier

Connector Part Information |

• | F 2-33

• | 2 Way Female

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
X | BRN | X16 | B+ When Defogger is ON
Y | RED/WHT | AM42 | Radio ON Signal

#### Radio, AM/FM Stereo and Clock and Tape Player and Compact Disk Player (Bose System)

Connector Part Information |

• | 12110115

• | ASM 32F M/P 100 (DK BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
E1 | YEL | B20 | Sound Processor Signal
E2-E4 | -- | -- | Not Used
E5 | GRY/YEL | RB40 | Illumination Signal
E6-E11 | -- | -- | Not Used
E12 | GRN | M92 | LH Negative Output
E13 | BRN/GRN | XM92 | LH Positive Output
E14 | BLK | S47 | Shield Wire
E15 | BLK | S46 | Shield Wire
E16 | BLK | F40 F49 | Ground to G201
F1 | RED | A52 | B+ from Multifunction Relay K134
F2 | -- | -- | Not Used
F3 | RED/WHT | AM110 AM116 | Radio ON Signal
F4 | GRY/GRN | RU72 | B+ from Fuse #26
F5 | BLK | F49 | Ground to G201
F6 | BRN/WHT | XM45 | Serial Data (Class 2)
F7 | -- | -- | Not Used
F8 | BLU/RED | PA101 | Remote Control Signal
F9 | BLK | F899 | Remote Control Signal
F10 | -- | -- | Not Used
F11 | BLK | S45 | Shield Wire
F12 | WHT | M90 | Chime Positive Output (Not Used)
F13 | BRN/WHT | XM93 | Chime Negative Output (Not Used)
F14 | WHT | M91 | RH Negative Output
F15 | BRN/WHT | XM91 | RH Positive Output
F16 | -- | -- | Not Used

#### Radio Speaker Amplifier (Bose System)

Connector Part Information |

• | ZF 25-1

• | 25 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRN | U3 | RH Rear Speaker Signal Output
2 | BRN/GRN | XU3 | RH Rear Speaker Signal Output
3 | BRN/BLU | XP12 | LH Front Negative Input
4 | BRN/YEL | XB12 | RH Front Negative Input
5 | BRN/GRN | XU12 | LH Rear Negative Input
6 | BRN/WHT | XM10 | RH Rear Negative Input
7 | WHT | M9 | RH Rear Positive Input
8 | GRN | U11 | LH Rear Positive Input
9 | YEL | B11 | RH Front Positive Input
10 | BLU | P11 | LH Front Positive Input
11-12 | -- | -- | Not Used
13 | RED | A200 | B+ from Fuse #6
14 | WHT | M3 | LH Rear Speaker Signal Output
15 | BRN/WHT | XM3 | LH Rear Speaker Signal Output
16 | BRN/BLU | XP2 | LH Front Door Speaker Output
17 | BLU | P2 | LH Front Door Speaker Output
18 | YEL | B4 | RH Front Door Speaker Output
19 | BRN/YEL | XB11 | RH Front Door Speaker Output
20 | GRN | U43 | LH Rear Door Speaker Output
21 | BRN/GRN | XU43 | LH Rear Door Speaker Output
22 | WHT | M43 | RH Rear Door Speaker Output
23 | BRN/WHT | XM43 | RH Rear Door Speaker Output
24 | BLK | F90 | Ground
25 | RED | A150 | Amp Enable Input

#### Sound Processor Interface Connector C1

Connector Part Information |

• | 12110207

• | ASM 32F M/P 100 (LT BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1-D1 | -- | -- | Not Used
D2 | RED | A150 | Amp Enable Output
D3-D11 | -- | -- | Not Used
D12 | BRN/WHT | XM90 | Chime Negative Input (Not Used)
D13 | WHT | M90 | Chime Positive Input (Not Used)
D14 | WHT | M16 | Cell Phone Negative Input
D15 | BRN/WHT | XM16 | Cell Phone Positive Input
D16 | -- | -- | Not Used

#### Sound Processor Interface Connector C2

Connector Part Information |

• | 12110206

• | ASM 24F M/P 100 (LT BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BLK | F151 | Ground
A2 | BRN/WHT | XM10 | RH Rear Negative Output
A3 | WHT | M9 | RH Rear Positive Output
A4 | BLK | SO3 | Shield Wire
A5 | BRN/GRN | XU12 | LH Rear Negative Output
A6 | GRN | U11 | LH Rear Positive Output
A7 | BLK | SO4 | Shield Wire
A8 | BRN/YEL | XM12 | RH Front Negative Output
A9 | YEL | B11 | RH Front Positive Output
A10 | BLK | SO1 | Shield Wire
A11 | BRN/BLU | XP12 | LH Front Negative Output
A12 | BLU | P11 | LH Front Positive Output
B1 | RED | A205 | B+ from Multifunction Relay K134
B2 | -- | -- | Not Used
B3 | BRN/WHT | XM45 | Serial Data (Class 2)
B4 | BRN/WHT | XM92 | LH Positive Input
B5 | WHT | M92 | LH Negative Input
B6 | WHT | M91 | RH Negative Input
B7 | BRN/WHT | XM91 | RH Positive Input
B8 | WHT | M45 | LH CD Positive Input
B9 | BLK | F45 | CD Common
B10 | -- | -- | Not Used
B11 | BLU | P45 | RH CD Positive Input
B12 | BLK | SO2 | Shield Wire

#### Steering Wheel Radio Control Switch

Connector Part Information |

• | ZPF 4-50

• | 4 Way Female

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | R1 | LED Output Control
B | BLU/RED | PA101 | Steering Wheel Switch Input
C | -- | -- | Not Used
D | BRN | X1 | Ground