For 1990-2009 cars

### Removal Procedure

1. Remove the heads from the lock housing shear bolts (1) by using a 6.5 mm drill bit (2).
2. Remove the lock housing (3) from the steering column housing assembly (1).
3. Remove the shear bolts (2) from the lock housing (3) using locking type pliers.

### Installation Procedure

1. Place lock in the RUN position.
2. Install the lock housing (2) onto the steering column housing assembly (3).
3. Install the new shear bolts (1) into the lock housing (2).

Tighten
The new shear bolts (1) until the heads separate from the shear bolt bodies.