For 1990-2009 cars

### Removal Procedure

1. Mark the position of the striker.
2. Remove the striker screws.
3. Remove the striker.
4. Remove the spacers, if equipped.

### Installation Procedure

1. Install any spacers that were removed.
2. Install the striker at the matchmark.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the striker screws.

Tighten
Tighten the door lock striker screws to 20 N·m (15 lb ft).

4. Clean off the matchmark.
5. Adjust the striker if neccessary. Refer to Rear Side Door Lock Striker Adjustment .