For 1990-2009 cars

### Removal Procedure

1. Remove the glass panel. Refer to Sunroof Glass Panel Replacement
2. Remove the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
3. Remove the sunroof actuator. Refer to Sunroof Actuator Replacement
4. Remove the water gutter. Refer to Water Gutter Replacement
5. Remove the sunscreen. To remove the suncreen, push in on the slide until they release from the tracks.

### Installation Procedure

1. Install the sunscreen. To install the sunscreen, snap in both sides to the track.
2. Install the water gutter. Refer to Water Gutter Replacement
3. Install the sunroof actuator. Refer to Sunroof Actuator Replacement
4. Install the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
5. Install the glass panel. Refer to Sunroof Glass Panel Replacement