For 1990-2009 cars

### Removal Procedure

Important: The cover cannot be removed until the mirror is removed for the windshield support.

1. Perform the following steps to remove the inside rearview mirror (automatic memory):

1.1. | Rock the mirror from side to side.

1.2. | Carefully pull the mirror down firmly.

1.3. | Do NOT pull rearward on the mirror while removing the mirror or damage to the support and/or windshield will occur.

2. Remove the inside rearview mirror electrical connector (2).
3. Remove the inside rearview mirror support (1).
4. Unsnap the inside rearview mirror base cover.

### Installation Procedure

1. Install the inside rearview mirror base cover.
2. Install the inside rearview mirror electrical connector (2).
3. Perform the following steps to install the inside rearview mirror:

3.1. | Center the bottom of the inside rearview mirror to the lower part of the support.

3.2. | Rock the inside rearview mirror from side to side while pushing upward firmly. Take care not to damage the windshield.

3.3. | Do NOT pull rearward on the mirror while installing the mirror or damage to the support and/or windshield will occur.

3.4. | An audible click is heard when the inside rearview mirror is fully seated.

4. Snap the inside rearview mirror base cover to the inside rearview mirror.