For 1990-2009 cars

### Removal Procedures

1. Release the rear seat belt center latch from the buckle.
2. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
3. Remove the lower rear seat belt retractor bolt.
4. Remove the bolt cover from the rear shoulder belt guide adjuster.
5. Remove the bolt from the rear seat belt shoulder belt guide adjuster.
6. Remove the outer seat back cushion. Refer to Seat Back Cushion Replacement - Rear Outer in Seats.
7. Remove the bolt from the rear seat shoulder belt retractor.
8. Remove the rear seat belt shoulder belt retractor.

### Installation Procedure

1. Install the rear seat shoulder belt retractor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt to the rear seat shoulder belt retractor.

Tighten
Tighten the rear seat belt retractor bolt to 35 N·m (26 lb ft).

3. Install the outer seat back cushion. Refer to Seat Back Cushion Replacement - Rear Outer in Seats.
4. Install the bolt to the rear seat shoulder belt guide adjuster.

Tighten
Tighten the rear seat shoulder guide adjuster bolt to 35 N·m (26 lb ft).

5. Install the bolt cover to the rear shoulder belt guide adjuster.
6. Install the lower rear seat shoulder belt retractor bolt.

Tighten
Tighten the lower rear seat shoulder belt bolt to 35 N·m (26 lb ft).

7. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
8. Reconnect the rear seat center shoulder belt latch to buckle.