For 1990-2009 cars

Causes | Action
--- | ---
The Selector Lever is in Position 1. | Adjust the Selector Lever Position Switch/Shift Linkage.
An incorrectly adjusted Selector Level Position Switch/Shift Linkage. | Refer to DTC P0753 1-2/3-4 Shift Solenoid Circuit Electrical .
A blocked Solenoid Valve for the 1-2/3-4 Shift or the On-Off valve in the Valve Body Assembly. |

1. Search for the blocked part.
2. Replace the blocked part.

Loss of fluid in Clutch C2 or in the Fluid Circuit. Only Recognizable upon Transmission removal and disassembly. |

1. Search for the leaking part.
2. Replace the leaking part.