For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the front fascia. Refer to Front Bumper Fascia Replacement
3. Remove the front bumper fascia support right side (1), center (2) and left side (3).

### Installation Procedure

1. Install the front bumper fascia support right side (1), center (2) and left side (3).
2. Install the front fascia. Refer to Front Bumper Fascia Replacement
3. Lower the vehicle.