For 1990-2009 cars

## Side Marker Lamp Replacement Front

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Access the bulb socket from under the front fascia to remove the bulb socket from the front sidemarker lamp.
3. Perform the following steps to remove the sidemarker lamp:

3.1. | Depress the clip on the sidemarker lamp.

3.2. | Angle the front sidemarker lamp out of the front fascia to remove the front sidemarker lamp. Ensure to not damage the pivot tab opposite the clip.

### Installation Procedure

1. Insert the pivot tab end of the front sidemarker lamp into the front fascia to snap in place.
2. Install the bulb socket to the front sidemarker lamp.
3. Lower the vehicle.

## Side Marker Lamp Replacement Rear

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Depress the clip on the rear sidemarker lamp from under the rear fascia.
3. Angle the rear sidemarker lamp out of the rear fascia. Ensure not to damage the pivot tab opposite the lamp clip.
4. Remove the bulb socket from the rear sidemarker lamp.

### Installation Procedure

1. Install the bulb socket to the rear sidemarker lamp.
2. Insert the pivot tab end into the rear fascia.
3. Snap the rear sidemarker lamp into place.
4. Lower the vehicle.