For 1990-2009 cars

### Removal Procedure

1. Remove the sunroof actuator. Refer to Sunroof Actuator Replacement
2. Remove the water gutter. Refer to Water Gutter Replacement
3. Remove the screw from the sunroof actuator cable stop.
4. Remove the sunroof actuator cable stop from the sunroof actuator.
5. Remove the slide and/or the guide from the sunroof actuator.
6. Remove the sunroof guide.

### Installation Procedure

1. Install the sunroof guide.
2. Install the slide and/or guide to the sunroof actuator.
3. Connect the sunroof actuator cable stop to the sunroof actuator.
4. Install the screw to the sunroof actuator cable stop.
5. Install the water gutter. Refer to Water Gutter Replacement .
6. Install the sunroof actuator. Refer to Sunroof Actuator Replacement .