For 1990-2009 cars

### Removal Procedure

1. Disable SIR system, if equipped with inflatable restraint side impact system. Refer to Disabling the SIR System in Restraints.
2. Front door window in the up position.
3. Remove front door trim panel. Refer to Front Side Door Trim Panel Replacement .
4. Remove front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Remove inflatable restraint side impact sensor mounting plate, if equipped. Refer to SIR Sensor Mounting Plate Replacement - Front Door .
6. Remove front door window guide screws.
7. Remove front door window guide.

### Installation Procedure

1. Install front door window guide.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install front door window guide screws.

Tighten
Tighten Window Guide Screws until fully seated and but not stripped.

3. Install inflatable restraint side impact sensor mounting plate, if equipped. Refer to SIR Sensor Mounting Plate Replacement - Front Door .
4. Install front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install front door trim panel. Refer to Front Side Door Trim Panel Replacement .
6. Enable SIR system, if equipped with inflatable restraint side impact system. Refer to Enabling the SIR System in SIR.