For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Disabling the SIR System in Restraints.
2. Remove the trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the trim panel retaining block. Refer to Front Side Door Trim Panel Bracket Replacement .
4. Remove the radio front side door speaker screws (1).
5. Remove the front door speaker.
6. Disconnect the speaker connector.
7. Starting at the top, pull downward on the water deflector in order to remove from the door edges.
8. Unroute the electrical connectors from the water deflector.

### Installation Procedure

1. Install the front door speaker.
2. Connect the speaker connector.
3. Install the speaker screws (1) until fully seated and not stripped.
4. Route the electrical connectors through the water deflector.
5. Install the water deflector to the door.
6. Install the trim retaining block. Refer to Front Side Door Trim Panel Bracket Replacement .
7. Install the trim panel. Refer to Front Side Door Trim Panel Replacement .
8. Enable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Enabling the SIR System in Restraints.