For 1990-2009 cars

### Removal Procedure

1. Twist and pull off the radio front side door tweeter speaker from the door pillar.
2. Disconnect the tweeter speaker connector.
3. Remove the tweeter speaker from the grille.
4. Pry of the assist handle front molding using a flat bladed plastic tool.
5. Remove door inside handle bezel by unsnapping.
6. Remove front screw trim cap.
7. Remove the assist handle screws.
8. Front door power door lock switch. Refer to Door Lock Switch Replacement
9. Disconnect outside power mirror switch electrical connector.
10. Remove the assist handle.

### Installation Procedure

1. Install the assist handle.
2. Front door power door lock switch. Refer to Door Lock Switch Replacement
3. Connect outside power mirror switch connector.
4. Install the assist handle screws.
5. Snap on the cover.
6. Install the tweeter to the door.
7. Connect the tweeter connector.
8. Snap the grille into place in the door pillar.