For 1990-2009 cars

### Removal Procedure

1. Depress the rear section of the sidemarker lamp and slide rearward.
2. Remove the front sidemarker lamp from the fascia.
3. Disconnect the electrical connector.
4. Remove the bulb socket by twisting the socket.
5. Remove the bulb from the bulb socket.

### Installation Procedure

1. Install the bulb to the bulb socket.
2. Install the bulb socket to the front sidemarker lamp.
3. Connect the electrical connection.
4. Insert the pivot tab end of the front sidemarker lamp into the front fascia to snap in place.