For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the differential with a transmission jack (1).
3. Remove the ABS sensor connectors (2).
4. Remove the differential support bracket bolts (1) from the differential support bracket (2).
5. Remove the rear differential bushing bolts (1) from the differential.

Important: The differential may be lowered slightly (4 to 5 inches) without the removal of the wheel drive shafts or the propeller shaft from the differential. This provides sufficient clearance to remove the differential housing cover.

6. Lower the differential slightly.
7. Place a drain pan underneath the differential.
8. Remove the differential housing cover bolts (1).
9. Remove the differential housing cover.
10. Clean the sealing surfaces on the differential housing.
11. Clean the sealing surfaces on the differential housing cover.
12. Remove the ABS sensor bolts from the cover.
13. Remove the ABS sensors from the cover.

### Installation Procedure

1. Install the ABS sensors to the cover.
2. Install the ABS sensor bolts to the cover.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the ABS sensor bolts to 7 N·m (62 lb in).

3. Coat the sealing surfaces uniformly with sealant, GM P/N 12346141 or equivalent.
4. Install the differential housing cover to the differential housing.
5. Install the differential housing cover bolts (1).

Tighten
Tighten the differential housing cover bolts (1) to 60 N·m (44 lb ft).

6. Raise the differential into place.
7. Install the differential support bracket bolts (1) to the differential support bracket (2).

Tighten
Tighten the differential support bracket bolts to 90 N·m (66 lb ft) + 38 degrees.

8. Install the differential bushing bolts (1) to the differential.

Tighten
Tighten the differential bushing bolts (1) to 100 N·m (74 lb ft).

9. Install the ABS sensor connectors (2).
10. Remove the transmission jack (1).
11. Refill the differential with proper lubricant. Refer to Lubricant Level Check .
12. Lower the vehicle.
13. Test drive the vehicle.
14. Inspect the vehicle for leaks.