For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system If equipped with the SIR side impact system. Refer to Disabling the SIR System in Restraints.
2. Disconnect the rubber conduit from door and pillar.
3. Loosen the plastic-type nut located on conduit closest to the door.
4. Grasp the conduit close to the end being removed.
5. Using a turning/pulling motion, remove the conduit.
6. Disconnect the wiring harness connectors.

### Installation Procedure

1. Connect the wiring harness connectors.
2. Install the conduit using a turning-pushing motion into the door and the pillar.
3. Using a turning/push motion, install the conduit to the door and pillar.
4. Tighten the plastic-type nut located on conduit closest to the door.
5. Enable the SIR system If equipped with the SIR side impact system. Refer to Enabling the SIR System in Restraints.