For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Press the LH front side door lock switch to the LOCK position.
2. Press the LH front side door lock switch to the UNLOCK position.

• | All side door lock actuators activate and lock all of the doors.

• | All side door lock actuators activate and unlock all of the doors.

All of the actuators do not activate. Refer to Door Lock Inoperative for diagnosis.

2 |

1. Turn the ignition switch to the ON position.
2. Ensure that the transmission is in the PARK position.
3. Press and release the rear compartment lid release switch.

The rear compartment lid lock release actuator activates and opens the rear compartment lid.

The rear compartment lid lock release actuator is inoperative. Refer to Rear Compartment Lid Release Inoperative for diagnosis.

3 | Press and release the fuel tank filler door lock release button on the portable transmitter (KEY FOB). | The fuel tank filler door lock actuator activates and opens the fuel tank filler door. | The fuel tank filler door lock actuator is inoperative. Refer to Fuel Filler Door Release Inoperative for diagnosis.
4 | Press and release the rear compartment lid release button on the portable transmitter (KEY FOB). | The rear compartment lid release actuator activates and opens the rear compartment lid. | The rear compartment lid lock release actuator is inoperative. Refer to Rear Compartment Lid Release Inoperative for diagnosis.
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.