For 1990-2009 cars

### Removal Procedure

1. Remove the console. Refer to Console Replacement in Instrument Panel, Gages and Console.
2. Remove the I/P accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gages and Console.
3. Remove the screws that retain the radio control to the I/P center support bracket.
4. Begin to remove the radio control from the center support bracket enough to access the connectors at rear of the radio control.
5. Disconnect the electrical/audio and coaxial cable connectors from the radio control.
6. Remove the radio control.

### Installation Procedure

1. Connect the electrical/audio and coaxial cable connectors to the radio control.
2. Install the radio control into position in the I/P center support bracket.

Align the radio control locator tab into the locator hole in the center support bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the radio control retaining screws.

Tighten
Tighten the retaining screws to 2.5 N·m (22 lb in).

4. Install the I/P accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gages and Console.
5. Install the console. Refer to Console Replacement in Instrument Panel, Gages and Console.
6. Install the scan tool.
7. Select RADIO THEFT from the SPECIAL FUNCTIONS menu.
8. Follow the instructions on the screen.