For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove trim panel retaining block. Refer to Rear Side Door Trim Panel Bracket Replacement .
3. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Remove the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
5. Remove the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
6. Remove the door lower weatherstrip. Refer to Rear Side Door Bottom Auxiliary Sealing Strip Replacement .
7. Remove the door vent window and division channel. Refer to Rear Side Door Stationary Window and Front Channel Replacement .
8. Remove the door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement .
9. Remove the door window up stop. Refer to Rear Side Door Window Stop Bumper Replacement .
10. Remove the door window regulator and motor. Refer to Rear Side Door Window Regulator Replacement .
11. Remove the door window. Refer to Rear Side Door Window Replacement .
12. Remove the door upper sealing strip. Refer to Rear Door Upper Sealing Strip Replacement .
13. Remove the speaker. Refer to Radio Rear Speaker Replacement in Entertainment.
14. Remove the inside door handle. Refer to Rear Side Door Inside Handle Replacement .
15. Remove the door lock. Refer to Rear Door Lock Replacement .
16. Remove the door outside handle. Refer to Rear Side Door Outside Handle Replacement .
17. Remove the side door molding. Refer to Door Body Side Molding Replacement in Exterior Trim.
18. Remove the door check link. Refer to Rear Side Door Check Link Replacement .
19. Remove the door rubber conduit. Refer to Rear Side Door Conduit Replacement .
20. Remove the door. Refer to Rear Side Door Removal .

### Installation Procedure

1. Install the door. Refer to Rear Side Door Removal .
2. Install the door rubber conduit. Refer to Rear Side Door Conduit Replacement .
3. Install the door check link. Refer to Rear Side Door Check Link Replacement .
4. Install the side door molding. Refer to Door Body Side Molding Replacement in Exterior Trim.
5. Install the door window. Refer to Rear Side Door Window Replacement .
6. Install the door outside handle. Refer to Rear Side Door Outside Handle Replacement .
7. Install the door lock. Refer to Rear Door Lock Replacement .
8. Install the inside door handle. Refer to Rear Side Door Inside Handle Replacement .
9. Install the speaker. Refer to Radio Rear Speaker Replacement in Entertainment.
10. Install the door upper sealing strip. Refer to Rear Door Upper Sealing Strip Replacement .
11. Install the door window. Refer to Rear Side Door Window Replacement .
12. Install the door window regulator and motor. Refer to Rear Side Door Window Regulator Replacement .
13. Install the door window up stop. Refer to Rear Side Door Window Stop Bumper Replacement .
14. Install the door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement .
15. Install the door lower weatherstrip. Refer to Rear Side Door Bottom Auxiliary Sealing Strip Replacement .
16. Install the door vent window division channel. Refer to Rear Side Door Stationary Window and Front Channel Replacement .
17. Install the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
18. Install the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
19. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
20. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .