For 1990-2009 cars

#### Heated Outside Rearview Mirror and Rear Window Defogger Relay (K35)

Connector Part Information |

• | ZF 6-14

• | 8-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X84 | Ignition 1 Voltage
2 | RED | A18 | Battery Positive Voltage
3 | -- | -- | Not Used
4 | BLK/WHT | FM14 | Heated Outside Rearview Mirrors and Rear Window Defogger Relay Control Circuit
5 | BLK/WHT | FM10 | HTD MIRROR Fuse Supply Voltage
6 | BLK | F84 | Ground
7 | -- | -- | Not Used
8 | BRN | X15 | Rear Window Defogger Supply Voltage

#### Inside Rearview Mirror (W/Memory)

Connector Part Information |

• | F 12-3

• | 12-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLU/RED | PA60 | Inside Rearview Mirror Motor Vertical Control
2 | BLU/WHT | PM60 | Inside Rearview Mirror Motor Horizontal Control
3 | BLK/RED | FA70 | Mirror Motor Control
4 | BRN | X70 | 5-Volt Reference
5 | BLK/BRN | FX70 | Low Reference
6 | GRY/YEL | RB60 | Inside Rearview Mirror Vertical Position Sensor Signal
7 | GRY/BLK | RF60 | Inside Rearview Mirror Horizontal Position Sensor Signal
8 | BLK | F915 | Ground
9 | BRN/BLU | XP900 | Interior Lamp Control
10 | WHT/BLK | MF900 | Backup Lamp Supply Voltage
11 | BRN | X900 | Ignition 1 Voltage
12 | -- | -- | Not Used