For 1990-2009 cars

### Circuit Description

The LEVELING indicator lamp is activated by the automatic level control (ALC) sensor whenever a compress cycle is requested. The sensor provides a switched path to ground. The sensor will flash the lamp when certain DTCs are detected. The sensor will not flash the lamp when this DTC is set.

### Conditions for Setting the DTC

The DTC will set when the sensor detects that the lamp output is not pulled down to ground when the sensor output is active and the ignition signal is high.

### Action Taken When the DTC Sets

• | The sensor's discrete low side output drive for the lamp is disabled.

• | The sensor continuously attempts to recover from the fault.

• | The LEVELING indicator lamp will not flash.

### Conditions for Clearing the DTC

• | A current DTC becomes history when conditions for the fault are no longer present and the ignition cycles from OFF to ON.

• | A history DTC will clear after 20 ignition cycles.

• | Using a scan tool.

### Diagnostic Aids

Check for the following conditions if a history or intermittent DTC is indicated:

• | A damaged wiring harness. Inspect the wiring harness for damage. If the wiring harness appears to be in good condition, observe the display on the DMM while moving the connectors and wiring harnesses related to the circuits. A change in the DMM display during this test will indicate the location of the fault.

• | For additional information, refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

### Test Description

The number(s) below refer to the step number(s) on the diagnostic table.

1. Tests for a short to voltage in the control circuit of the LEVELING indicator lamp.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Automatic Level Control (ALC) Diagnostic System Check? | -- | Go to Step 2 | Go to Automatic Level Control Diagnostic System Check
2 |

1. Disconnect the automatic level control (ALC) sensor connector.
2. Measure the voltage between the ALC sensor connector terminal G and ground.

Is the voltage reading greater than the specified value?

0.1 V

Go to Step 3

Go to Step 4

3 | Repair a short to voltage in the control circuit of the LEVELING indicator lamp. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Step 5 | --
4 | Replace the ALC sensor. Refer to Automatic Level Control Sensor Replacement . Is the repair complete? | -- | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2