For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .

Remove the front seat cushion pad and the cover can be removed as an assembly when replacing front seat cushion frame.

3. Remove the pivot pin bolt from the front seatback.

These pivot pin bolts are located on the inner and outer sides of the seat cushion frame.

4. Remove the seat adjuster bolts.
5. Remove the front seat cushion frame.

### Installation Procedure

1. Install the front seat cushion frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the seat adjuster bolts.

Tighten
Tighten the seat adjuster bolts to 25 N·m (19 lb ft).

3. Install the pivot pin bolts to the front seatback.

Tighten
Tighten the pivot pin bolts to 20 N·m (15 lb ft).

4. Install the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
5. Install the front seat. Refer to Seat Replacement .