For 1990-2009 cars

Problem | Action
--- | ---
The springs are broken or sagging. | Inspect and repair as necessary. Refer to Trim Height Inspection .
The stabilizer shaft is loose or disconnected. | Inspect the stabilizer shaft links and insulators for damage. Repair or replace as necessary.

• | For the stabilizer shaft link replacement. Refer to Stabilizer Shaft Link Replacement in Front Suspension or Stabilizer Shaft Link Replacement in Rear Suspension.

• | For the stabilizer shaft insulator replacement. Refer to Stabilizer Shaft Replacement in Front Suspension or Stabilizer Shaft Insulator Replacement in Rear Suspension.

The struts are worn. | Inspect and repair as necessary. Refer to Strut, Strut Component, and Spring Replacement in Front Suspension.
The vehicle is overloaded. | Reduce the vehicle load. Refer to Tire Placard in General Information.
The tire pressure(s) is incorrect. | Inflate the tire(s) to proper specifications. Refer to Tire Inflation Pressure Specifications in Maintenance and Lubrication.