For 1990-2009 cars

### Removal Procedure

1. Set the parking brake and move the shifter selector to the full rear position.
2. Open the ashtray.
3. Release the outer tray cover from the right side of the assembly and remove.
4. Remove the screw from the rear of the ashtray.
5. Remove the ashtray from the instrument panel.

### Installation Procedure

1. Install the ashtray to the instrument panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screw to the rear of the ashtray.

Tighten
Tighten the screw to 2 N·m (18 lb in).

3. Install the outer tray cover to the ashtray assembly.
4. Close the ashtray.

Install the shifter selector to the full forward position and release the parking brake.