For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the rear seatback cushion. Refer to Rear Seat Back Replacement .
3. Remove the rear seatback pad.

### Installation Procedure

1. Install the rear seatback pad.
2. Install the rear seatback cushion. Refer to Rear Seat Back Replacement .
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .