For 1990-2009 cars

### Driver's Side Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement
2. Remove the driver side sound insulator retainers.
3. Remove the driver side sound insulator.

### Driver's Side Installation Procedure

1. Install the driver side sound insulator.
2. Install the driver side sound insulator retainers.
3. Install the knee bolter. Refer to Knee Bolster Replacement

### Passenger Side Removal Procedure

1. Remove the passenger side sound insulator retainers.
2. Remove the passenger side sound insulator.

### Passenger Side Installation Procedure

1. Install the passenger side sound insulator.
2. Install the passenger side sound insulator retainers.