For 1990-2009 cars

Check the marks on the fluid level indicator integrated with the reservoir cap to determine fluid level.

Notice: When adding fluid or making a complete fluid change, always use the proper power steering fluid. Failure to use the proper fluid will cause hose and seal damage and fluid leaks.

The fluid should be between the upper level indicator line and the lower indicator line with the power steering fluid warmed up to about 77°C (170°F) or hot to the touch. The fluid level should be at or just below the lower indicator line if the fluid level is cool, about 21°C (70°F).