For 1990-2009 cars

## Speaker Replacement Door Tweeter

### Removal Procedure

1. Twist and pull off the radio front side door tweeter grille from the door pillar.
2. Disconnect the tweeter connector.
3. Remove the tweeter from the grille.

### Installation Procedure

1. Install the tweeter to the grille.
2. Connect the tweeter connector.
3. Snap the grille into place in the door pillar.

## Speaker Replacement Front Door Speaker

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Remove the radio front side door speaker screws (1).
3. Disconnect the speaker connector.

### Installation Procedure

1. Connect the speaker connector.
2. Install the speaker screws (1) until fully seated and not stripped.
3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.

## Speaker Replacement Rear Door Speaker

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement in Doors.
2. Remove the radio rear side door speaker screws (1).
3. Disconnect the speaker connector.

### Installation Procedure

1. Connect the speaker connector.
2. Install the speaker screws (1) until fully seated and not stripped.
3. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement in Doors.

## Speaker Replacement Rear Speaker

### Removal Procedure

1. Remove the rear seat to rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.
2. Disconnect the radio rear speaker connector (1).
3. Remove the speaker screws (1).
4. Remove the speaker (2) with the baffle from the rear parcel shelf.

### Installation Procedure

1. Install the speaker (2) with the baffle at the rear parcel shelf.
2. Install the speaker screws (1) until fully seated and not stripped.
3. Connect the speaker connector (1).
4. Install the rear seat to rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.