For 1990-2009 cars

### Removal Procedure

1. Slide the sunscreen all the way rearward.
2. Open the glass panel halfway.
3. Remove the screws from the brush cover along the front edge.
4. Unclip the brush cover from both rear corners.
5. Open the glass panel all the way.
6. Remove the brush cover through the glass panel opening.

### Installation Procedure

1. Install the brush cover through the glass panel opening.
2. Close the glass panel half way.
3. Clip the brush cover to both rear corners.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the screws to the brush cover along the front edge.

Tighten
Tighten the brush cover screws until fully seated not stripped.

5. Close the glass panel.
6. Slide the sunscreen closed.