For 1990-2009 cars

### Removal Procedure

1. Remove the rear seatback cushion. Refer to Rear Seat Back Replacement .
2. Remove the rear seatback pad. Refer to Rear Seat Back Cushion Pad Replacement .
3. Remove seatback cushion frame.

### Installation Procedure

1. Install the seatback cushion frame.
2. Remove the rear seatback pad. Refer to Rear Seat Back Cushion Pad Replacement .
3. Install the rear seatback cushion. Refer to Rear Seat Back Replacement .