For 1990-2009 cars

### Removal Procedure

1. Disable SIR system If equipped with SIR side impact system. Refer to Disabling the SIR System in Restraints.
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement
3. Remove the trim panel retaining block. Refer to Front Side Door Trim Panel Bracket Replacement
4. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement
5. Remove the Inflatable restraint side impact sensor mounting plate if equipped. Refer to SIR Sensor Mounting Plate Replacement - Front Door
6. Remove the front door inner belt sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement
7. Remove the outside rearview mirror. Refer to Power Mirror Replacement
8. Remove the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement
9. Remove the upper sealing strip. Refer to Front Side Door Upper Auxiliary Sealing Strip Replacement
10. Remove the front door window weatherstrip. Refer to Front Side Door Window Weatherstrip Replacement
11. Remove the front door window up stop. Refer to Front Side Door Window Stop Bumper Replacement
12. Remove the front door window regulator and motor. Refer to Front Side Door Window Regulator Replacement
13. Remove the front door window. Refer to Front Side Door Window Replacement
14. Remove the front door speaker. Refer to Speaker Replacement in Entertainment.
15. Remove the front door inside handle. Refer to Front Side Door Inside Handle Replacement
16. Remove the front door lock. Refer to Front Side Door Lock Replacement
17. Remove the front door outside handle. Refer to Front Side Door Outside Handle Replacement
18. Remove the front door body side molding. Refer to Door Body Side Molding Replacement
19. Remove the front door check link. Refer to Front Side Door Check Link Replacement
20. Remove the front door rubber conduit. Refer to Front Side Door Conduit Replacement
21. Remove the front door electrical connectors and harness from the door.
22. Remove the front door. Refer to Door Removal - Front

### Installation Procedure

1. Install the front door. Refer to Door Removal - Front
2. Install the front door electrical connectors and harness from the door.
3. Install the front door rubber conduit. Refer to Front Side Door Conduit Replacement
4. Install the front door check link. Refer to Front Side Door Check Link Replacement
5. Install the front door body side molding. Refer to Door Body Side Molding Replacement
6. Install the front door outside handle. Refer to Front Side Door Outside Handle Replacement
7. Install the front door lock. Refer to Front Side Door Lock Replacement
8. Install the front door inside handle. Refer to Front Side Door Inside Handle Replacement
9. Install the front door speaker. Refer to Speaker Replacement in Entertainment.
10. Install the front door window regulator and motor. Refer to Front Side Door Window Regulator Replacement
11. Install the front door window. Refer to Front Side Door Window Replacement
12. Install the front door window up stop. Refer to Front Side Door Window Stop Bumper Replacement
13. Install the front door window weatherstrip. Refer to Front Side Door Window Weatherstrip Replacement
14. Install the upper sealing strip. Refer to Front Side Door Upper Auxiliary Sealing Strip Replacement
15. Install the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement
16. Install the outside rearview mirror. Refer to Power Mirror Replacement
17. Install the front door inner belt sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement
18. Install the Inflatable restraint side impact sensor mounting plate if equipped. Refer to SIR Sensor Mounting Plate Replacement - Front Door
19. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement
20. Install the trim panel retaining block. Refer to Front Side Door Trim Panel Bracket Replacement
21. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement
22. Enable SIR system If equipped with SIR side impact system. Refer to Enabling the SIR System In Restraints.