For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement
2. Remove retainer rings form the seat cushion cover and from the frame.

Put down a protective cover to prevent damage to rear seat cushion cover.

3. Remove the rear seat cushion cover.
4. Unroute seat cushion heating element wiring from seat cushion pad.

### Installation Procedure

1. Route seat cushion heating element wiring through seat cushion pad.
2. Install the rear seat cushion cover.
3. Install the retainer rings to the rear seat cushion cover and to the frame.
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement