For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Disconnect the seat belt switch.
2. Turn ON the ignition, leaving the engine OFF.

Is the Fasten Seat Belt lamp illuminated?

--

Go to Step 3

Go to Step 4

3 | Replace the seat belt switch. Did you complete the replacement? | -- | Go to Step 5 | --
4 | Test the seat belt switch signal circuit for a short to ground (CKTs XF20 and XF21). Refer to Testing for Short to Ground in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 5 | Go to Step 6
5 | Verify the operation of the Fasten Seat Belt lamp. Is the Fasten Seat Belt lamp operating properly? | -- | System OK | --
6 |

1. Remove the instrument panel cluster. Refer to Instrument Cluster Replacement .
2. Remove and inspect the Fasten Seat Belt indicator bulb, located in the gauge cluster, for an open.

Did you find and correct the condition?

--

Go to Step 5

Go to Step 7

7 | Replace the gauge cluster. Did you complete the replacement? | -- | Go to Step 8 | --
8 | Test the gauge cluster functions. Do all gauge cluster functions operate properly? | -- | System OK | --