For 1990-2009 cars

#### Gauge Cluster Connector

Connector Part Information |

• | ZF 26 - 1

• | 26 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/YEL | XB3 | Washer Solvent Level Signal
2 | YEL/RED | BA2 | Brake Pad Wear Signal
3 | BRN/BLU | XP2 | Low Coolant Level Signal
4 | BRN/GRN | XU600 | Oil Level Signal
5 | RED | A900 | Fused ignition (terminal W)
6 | BLK | F8 | Ground
7-8 | -- | -- | Not Used
9 | BLU/RED | PA600 | Vehicle Speed Signal (oil pressure warning)
10-12 | -- | -- | Not Used
13 | GRN | U5 | Tach Signal (oil pressure warning)
14 | BRN/BLK | XF20 | Seat Belt Switch Signal
15 | BLU/GRN | PU1 | Oil Pressure Switch Signal
16 | GRY/WHT | RM900 | Headlamps ON Signal
17 | GRY/YEL | RB103 | Interior Lamps Dimming Signal
18 | BLU/WHT | PM1 | Generator Input Signal
19 | -- | -- | Not Used
20 | BRN | X70 | Fused Ignition Feed
21 | BRN/PPL | XY2 | ALC Sensor Signal
22 | RED | A16 | Fused Battery Feed
23 | BRN/BLU | XP840 | Security Lamp Signal
24 | BLK | F11 | Lamp Ground
25 | -- | -- | Not Used
26 | BLU/YEL | PB90 | Oil Pressure Sensor Signal

#### Headlamp Switch

Connector Part Information |

• | ZF 18-7

• | 18 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/GRN | RU70 | B+ from Fuse #26
2 | GRY/YEL | RB1 | Dimmer Output Signal
3 | BRN | X22 | B+ from Fuse #15
4 | BRN/RED | XA811 | Low Beam Relay Signal
5 | BRN/WHT | XM815 | Park Lamp Relay Signal
6 | YEL | B60 | Low Beam ON/OFF Signal
7 | RED/WHT | AM813 | Park Lamp ON/OFF Signal
8 | BRN/PPL | XY112 | Interior lamps ON/OFF signal
9 | RED/YEL | AB810 | TS ON/OFF Signal
10 | BLK/BLU | FP28 | Fog Lamp Switch Signal
11 | BLK/BRN | FX810 | TS Delay Signal
12 | BLK/PPL | FY810 | TS Return Signal
13 | BLK | F18 | Ground to G103
14 | YEL | B55 | B+ form Fuse #22
15 | -- | -- | Not used
16 | BRN/BLK | XF830 | TS Indicator
17 | RED | A5 | B+ from Fuse #8
18 | GRY/WHT | RM1 RM900 | Chime Control Signal

#### Ignition Switch and Lifting Magnet

Connector Part Information |

• | ZF6-5

• | 6 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A905 | B+ from fuse #24
2 | GRN | U900 | Brake to shift signal
U | BRN | X826 | B+ in the ON position
V | BRN | X1 | B+ in the ON or START position
W | RED | A19 | B+ when the key is inserted
Y | RED | A503 | B+ from fuse V4
Z | BLK/RED | FA700 | Starter solenoid signal

#### LH Front Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/WHT | RM2 | Door Open Signal
2 | GRY | R2 | Door Open Signal