For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Pull back the sealing strip on the RH of the air inlet grille.
3. Open the air inlet grille flap.
4. Release the pollen filter.
5. Pull the filter straight up in order to remove from the vehicle.

### Installation Procedure

1. Install the pollen filter.
2. Secure the filter tabs (1).
3. Close the air inlet grille flap.
4. Install the sealing strip.
5. Close the hood.