For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the seat adjuster. Refer to Power Seat Adjuster Mechanism Replacement .
3. Remove the seat adjuster actuator motor. Refer to Seat Adjuster Motor Replacement - Power .
4. Remove the driveshaft.

### Installation Procedure

1. Install the driveshaft.
2. Install the seat adjuster actuator motor. Refer to Seat Adjuster Motor Replacement - Power .
3. Install the seat adjuster. Refer to Power Seat Adjuster Mechanism Replacement .
4. Install the front seat. Refer to Seat Replacement .