For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment floor carpet. Refer to Rear Floor Trim Plate Replacement .
2. Remove the spare tire. Refer to Spare Wheel and Hold-Down Replacement .
3. Remove the screw retainers.
4. Remove the screws across the top of the panel.
5. Remove the rear trim panel.

### Installation Procedure

1. Install the rear trim panel.
2. Install the screws across the top of the panel.
3. Install the screw retainers.
4. Install the spare tire. Refer to Spare Wheel and Hold-Down Replacement .
5. Install the rear compartment floor carpet. Refer to Rear Floor Trim Plate Replacement .