For 1990-2009 cars

### Ride To Soft

• | Inspect for leaking struts or shock absorbers.

• | Inspect for incorrect springs.

• | Inspect for incorrect tire pressure(s).

• | Inspect for Automatic Level Control System not functioning properly.

### Ride To Harsh

• | Inspect for overinflated tires.

• | Inspect for Automatic Level Control System not functioning properly.

• | Inspect for incorrect front or rear springs.

• | Inspect for binding struts or shock absorbers.